No technical connection layaut

Moving back to the old configuration just connect cable 2 to 220 and cable 1 to Variac output

< Lamp PWR (200, 100, 40, Variac Volts)

< Lamp Fan (220 Volts)

FFLamp Voltages >

FF Lamp

Dome

Variac

To 220 V (32 Amp braker)

Adam6060

Trafo with 3 taps

Relays

Switch and Voltage Distribution Box

< Variac PWR 220V

< Variac output 0 - 220 Volts

..Switchable

(Main switch have to be always ON. There is no need to switch it off at the Dome FF end)

To LaSilla LAN

< Pwr 220V

(Adam-6060 ModBus connection)

1

2 1

ESO 220 DOME FLA T FIELD CONTROL PROCEDURE

1. Star ADAM tool fr om operation PC. (double click on ADAM icon) 2. Wait for sear ching device pr ocedur e be done successfully. 3. On the dir ectory tr ee look for sub-dir ectory 6060. Once you ther e on the right workspace will appear several buttons either for input or outputs commands, but the needed ones ar e DO0 DO1 DO2 DO3 4. Set digital output button DO3 OFF 5. Select voltage using buttons DO02, DO1, D00 accor ding to the following tables.

VARIAC is still connected as an option to set (manually) any other voltage. 6. FF LampOn by switching DO3 ON WARNING: DODO3 OFF before changing voltage. Also for safety during observation use the Dome Lamp Switch OFF on the EMERGENCY button Box.

Table 1: Voltage DO2 DO1 DO0 200 OFF OFF OFF 100 OFF OFF ON 40 ON OFF OFF VARIAC ON ON ON Table 2:

Voltage DO2 DO1 DO0 200 OFF ON OFF 100 OFF ON ON 40 ON OFF ON VARIAC ON ON OFF